{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["ETA","RBD","FTA","Parametere","IoT_GET"],"not_rendered":{"charts":0,"images":9,"macros":1,"external_links":1,"defined_names":52,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ETA","index":0,"n_rows":20,"n_cols":14,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
["¯ = Nei, ® = Ja"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Formel, Frekvens"]
["Ingen kjøling VV, f=",null,"TT, feiler, q=",null,null,"Operatør feiler, q=",null,null,null,null,null,"Ingen kjøling, F="]
[{"$f":"F_0","v":5.2151748295490089E-5},null,{"$f":"q_TT","v":6.9444444444444449E-3},null,null,{"$f":"1-90%","v":9.9999999999999978E-2},null,null,null,null,null,{"$f":"fInit*q_TT2*q_Op","v":3.6216491871868111E-8},null,{"$f":"ShowFormula(L4)","v":"=fInit*q_TT2*q_Op"}]
[{"$f":"ShowFormula(fInit)","v":"=F_0"},null,{"$f":"ShowFormula(q_TT2)","v":"=q_TT"},null,null,{"$f":"ShowFormula(q_Op)","v":"=1-90%"}]
[null,null,null,null,null,null,null,null,"P3 eller DM feiler, q=",null,null,"Ingen kjøling, F="]
[null,null,null,null,null,null,null,null,{"$f":"q_P3+q_DM","v":1.8749999999999999E-2},null,null,{"$f":"fInit*q_TT2*(1-q_Op)*q_SeaWater1","v":6.1115330033777453E-9},null,{"$f":"ShowFormula(L7)","v":"=fInit*q_TT2*(1-q_Op)*q_SeaWater1"}]
[null,null,null,null,null,null,null,null,{"$f":"ShowFormula(q_SeaWater1)","v":"=q_P3+q_DM"}]
[null,null,null,null,null,null,null,null,null,null,null,"Forsinket kjøling, F="]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"fInit*q_TT2*(1-q_Op)*(1-q_SeaWater1)","v":3.1983689384343532E-7},"(ii)",{"$f":"ShowFormula(L10)","v":"=fInit*q_TT2*(1-q_Op)*(1-q_SeaWater1)"}]
[]
[null,null,null,null,null,null,null,null,"P3 eller DM feiler, q=",null,null,"Ingen kjøling, F="]
[null,null,null,null,null,null,null,null,{"$f":"q_P3+q_DM","v":1.8749999999999999E-2},null,null,{"$f":"fInit*(1-q_TT2)*q_SeaWater2","v":9.7105468831446401E-7},null,{"$f":"ShowFormula(L13)","v":"=fInit*(1-q_TT2)*q_SeaWater2"}]
[null,null,null,null,null,null,null,null,{"$f":"ShowFormula(q_SeaWater2)","v":"=q_P3+q_DM"}]
[null,null,null,null,null,null,null,null,null,null,null,"Sjøvannskjøling, F="]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"fInit*(1-q_TT2)*(1-q_SeaWater2)","v":5.0818528688456946E-5},"(i)",{"$f":"ShowFormula(L16)","v":"=fInit*(1-q_TT2)*(1-q_SeaWater2)"}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"S ingen kjøling, F="]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"L7+L4+L13","v":1.0133827131897099E-6},"(iii)"]

{"sheet":"RBD","index":1,"n_rows":27,"n_cols":20,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Enhet","MTTF (år)","MTTF (t)","MDT (t)","t (t)","navn","p"]
["Lager moduler av hver grein, I og II, med strukturfunksjoner hhv ",null,null,null,null,null,null,null,null,null,null,null,null,"Pumpe, P1",1,{"$f":"O11*8760","v":8760},8,null,"P_P1",{"$f":"(P11)/(P11+Q11)","v":0.99908759124087587}]
[" og ",null,null,null,null,null,null,null,null,null,null,null,null,"Pumpe, P2",1,{"$f":"O12*8760","v":8760},8,null,"P_P2",{"$f":"(P12)/(P12+Q12)","v":0.99908759124087587}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Elektrisk motor, M1 ",2,17520,24,null,"P_M1",0.99863201094391241]
["For hele strukturen: ",null,null,null,null,null,null,null,null,null,null,null,null,"Elektrisk motor, M2",2,17520,24,null,"P_M2",0.99863201094391241]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Varmeveksler, VV",4,35040,48,null,"P_VV",0.99863201094391241]
["Innsatt: ",null,null,null,null,null,null,null,null,null,null,null,null,"Strømforsyning, S",5,43800,4,null,"P_S",0.99990868413843481]
[]
["Stryker potenser: "]
[]
[]
[]
["Systempålitelighet: "]
[]
[]
["Innsatt"]
["h(p)=",{"$f":"(P_P1*P_M1*P_S+P_P2*P_M2*P_S-P_P1*P_P2*P_M1*P_M2*P_S)*P_VV","v":{"$error":"#REF!"}}]
["1-h",{"$f":"1-B26","v":{"$error":"#REF!"}}]

{"sheet":"FTA","index":2,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Q0 - bidrag","Formel","F0 - bidrag","Formel"]
["Cut set(s) with 1 component"]
["   {S} ",{"$f":"q_S","v":9.1324200913242012E-5},{"$f":"ShowFormula(B5)","v":"=q_S"},{"$f":"lambda_S","v":2.2831050228310503E-5},{"$f":"ShowFormula(D5)","v":"=lambda_S"}]
["   {VV} ",{"$f":"q_VV","v":1.3698630136986301E-3},{"$f":"ShowFormula(B6)","v":"=q_VV"},{"$f":"lambda_VV","v":2.8538812785388127E-5},{"$f":"ShowFormula(D6)","v":"=lambda_VV"}]
[" ",null,"",null,""]
["Cut set(s) with 2 components ",null,"",null,""]
["   {P1,P2} ",{"$f":"q_P1*q_P2","v":8.3401096724421924E-7},"=q_P1*q_P2",{"$f":"lambda_P1*q_P2+q_P1*lambda_P2","v":2.0850274181105481E-7},"=lambda_P1*q_P2+q_P1*lambda_P2"]
["   {P1,M2} ",{"$f":"q_P1*q_M2","v":1.2510164508663289E-6},"=q_P1*q_M2",{"$f":"lambda_P1*q_M2+q_P1*lambda_M2","v":2.0850274181105481E-7},"=lambda_P1*q_M2+q_P1*lambda_M2"]
["   {M1,P2} ",{"$f":"q_M1*q_P2","v":1.2510164508663289E-6},"=q_M1*q_P2",{"$f":"lambda_M1*q_P2+q_M1*lambda_P2","v":2.0850274181105481E-7},"=lambda_M1*q_P2+q_M1*lambda_P2"]
["   {M1,M2} ",{"$f":"q_M1*q_M2","v":1.8765246762994934E-6},"=q_M1*q_M2",{"$f":"lambda_M1*q_M2+q_M1*lambda_M2","v":1.5637705635829111E-7},"=lambda_M1*q_M2+q_M1*lambda_M2"]
["Q0=",{"$f":"SUM(B5:B12)","v":1.4663997831571485E-3},"F0=",{"$f":"SUM(D5:D12)","v":5.2151748295490089E-5}]
["Q0× 8760 = timer per år =",{"$f":"B13*8760","v":12.84566210045662},null,{"$f":"D13*8760","v":0.45684931506849319},"(Frekvens per år)"]

{"sheet":"Parametere","index":3,"n_rows":10,"n_cols":8,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["Enhet","MTTF (år)","MDT (t)","t (t)","navn","l","navn","q"]
["Pumpe, P1",1,8,null,"lambda_P1",{"$f":"1/(8760*B2)","v":1.1415525114155251E-4},"q_P1",{"$f":"C2*F2","v":9.1324200913242006E-4}]
["Pumpe, P2",1,8,null,"lambda_P2",{"$f":"1/(8760*B3)","v":1.1415525114155251E-4},"q_P2",{"$f":"C3*F3","v":9.1324200913242006E-4}]
["Elektrisk motor, M1 ",2,24,null,"lambda_M1",5.7077625570776254E-5,"q_M1",1.3698630136986301E-3]
["Elektrisk motor, M2",2,24,null,"lambda_M2",5.7077625570776254E-5,"q_M2",1.3698630136986301E-3]
["Varmeveksler, VV",4,48,null,"lambda_VV",2.8538812785388127E-5,"q_VV",1.3698630136986301E-3]
["Strømforsyning, S",5,4,null,"lambda_S",2.2831050228310503E-5,"q_S",9.1324200913242012E-5]
["Pumpe P3",5,null,730,"lambda_P3",2.2831050228310503E-5,"q_P3",{"$f":"D8*F8/2","v":8.3333333333333332E-3}]
["Dieselmotor, DM",4,null,730,"lambda_DM",2.8538812785388127E-5,"q_DM",{"$f":"D9*F9/2","v":1.0416666666666666E-2}]
["Temperaturmåler, TT",6,null,730,"lambda_TT",1.9025875190258754E-5,"q_TT",6.9444444444444449E-3]

{"sheet":"IoT_GET","index":4,"n_rows":5,"n_cols":3,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["Name","Value","Description"]
["sjonFolder","https://folk.ntnu.no/jvatn/eLearning/DT/","Usually, do not update"]
["sjonName","sJonTest","Name of SJON file to use, without extension"]
["Par1_",2]
["Par2_",5]