{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["IoT_GET"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":47,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"IoT_GET","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["Name","Value","Description"]
["sjonFolder","https://jvatn.folk.ntnu.no/eLearning/DT/","Usually, do not update",null,"Digital twin"]
["sjonName","DT_Pump_Descriptive","Name of SJON file to use, without extension"]
["lambda_A",1.4999999999999999E-4,"Konstant sviktintensitet, aktiv pumpe"]
["lambda_S",5.0000000000000002E-5,"Konstant sviktintensitet, standbypumpe"]
["MDT",12,"Midlere nedetid ved svikt av aktiv pumpe"]
["C_U",25000,"Nedetidskostnad per time"]
["C_FT",2000,"Kostnad for funksjonstest"]
["C_T",50000,"Kostnad for \"trip\", dvs ved systemsvikt"]
["tau",1234.437744140625,"Intervall for funksjonstesting, standbypumpe",null,"Optimizer"]
["PFD",{"$f":"lambda_S*tau/2","v":3.0860943603515628E-2},{"$f":"_xlfn.FORMULATEXT(B11)","v":"=lambda_S*tau/2"}]
["MTTF_A",{"$f":"(1/lambda_A)/8760","v":0.76103500761035014},{"$f":"_xlfn.FORMULATEXT(B12)","v":"=(1/lambda_A)/8760"}]
["MTTF_S",{"$f":"(1/lambda_S)/8760","v":2.2831050228310503},"=(1/lambda_S)/8760"]
["q_A",{"$f":"lambda_A*MDT","v":1.8E-3},"=lambda_A*MDT"]
["Q_System",{"$f":"q_A*PFD","v":5.554969848632813E-5},"=q_A*PFD"]
["Nedetid",{"$f":"Q_System*8760","v":0.48661535874023443},"Timer per år"]
["F_system",{"$f":"lambda_A*PFD","v":4.6291415405273439E-6},"=lambda_A*PFD"]
["F per år",{"$f":"B17*8760","v":4.0551279895019533E-2},"Per år"]
["C_tau",{"$f":"C_FT/tau+C_U*Q_System+C_T*F_system","v":3.2403703493312856},"=C_FT/tau+C_U*Q_System+C_T*F_system"]
["C per år",{"$f":"B19*8760","v":28385.644260142064},"Per år"]
["msg","Veldig kort nedetid"]