{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["IoT_GET"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":57,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"IoT_GET","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
["Name","Value","Description"]
["sjonFolder","https://jvatn.folk.ntnu.no/eLearning/DT/","Usually, do not update",null,"Digital twin"]
["sjonName","DT_Pump_Predictive","Name of SJON file to use, without extension"]
["mu",0.05,"Drift"]
["sigma",0.15,"Standardavvik, inkrementer"]
["l",100,"Sviktgrense"]
["lambda_S",5.0000000000000002E-5,"Konstant sviktintensitet, standbypumpe"]
["MDT",24,"Midlere nedetid ved svikt av aktiv pumpe"]
["C_U",25000,"Nedetidskostnad per time"]
["C_FT",2000,"Kostnad for funksjonstest",null,"Optimizer"]
["C_T",50000,"Kostnad for \"trip\", dvs ved systemsvikt"]
["tau",1314.678955078125,"Intervall for funksjonstesting, standbypumpe"]
["x_t0",80,"Tilstand ved nåtidspunkt (t0)"]
["T_L",{"$f":"14*24","v":336},"Ledetid"]
["E(T)",{"$f":"l/mu","v":2000},{"$f":"_xlfn.FORMULATEXT(B15)","v":"=l/mu"}]
["SD(T)",{"$f":"SQRT(sigma^2*l/mu^3)","v":134.16407864998737},{"$f":"_xlfn.FORMULATEXT(B16)","v":"=SQRT(sigma^2*l/mu^3)"}]
["alpha",{"$f":"(l-x_t0)/mu","v":400},{"$f":"_xlfn.FORMULATEXT(B17)","v":"=(l-x_t0)/mu"}]
["beta",{"$f":"(l-x_t0)^2/sigma^2","v":17777.777777777777},"=(l-x_t0)^2/sigma^2"]
["F_T",{"$f":"cdfIG(T_L,alpha,beta)","v":0.13789907097816467},"=cdfIG(T_L,alpha,beta)"]
["PFD",{"$f":"lambda_S*tau/2","v":3.2866973876953129E-2},{"$f":"_xlfn.FORMULATEXT(B20)","v":"=lambda_S*tau/2"}]
["lambda_A",{"$f":"F_T/(E_T-alpha+T_L)","v":7.1228858976324724E-5},{"$f":"_xlfn.FORMULATEXT(B21)","v":"=F_T/(E_T-alpha+T_L)"}]
["MTTF_A",{"$f":"(1/lambda_A)/8760","v":1.6026544968170247},{"$f":"_xlfn.FORMULATEXT(B22)","v":"=(1/lambda_A)/8760"}]
["MTTF_S",{"$f":"(1/lambda_S)/8760","v":2.2831050228310503},"=(1/lambda_S)/8760"]
["q_A",{"$f":"lambda_A*MDT","v":1.7094926154317934E-3},"=lambda_A*MDT"]
["Q_System",{"$f":"q_A*PFD","v":5.6185849134241035E-5},"=q_A*PFD"]
["Nedetid",{"$f":"Q_System*8760","v":0.49218803841595149},"Timer per år"]
["F_system",{"$f":"lambda_A*PFD","v":2.3410770472600431E-6},"=lambda_A*PFD"]
["F per år",{"$f":"B27*8760","v":2.0507834933997979E-2},"Per år"]
["C_tau",{"$f":"C_FT/tau+C_U*Q_System+C_T*F_system","v":3.0429840354630593},"=C_FT/tau+C_U*Q_System+C_T*F_system"]
["C per år",{"$f":"B29*8760","v":26656.540150656398},"Per år"]
["msg","Veldig veldig sent"]