{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["From lecture","Parameters","FTA's","ETA"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"From lecture","index":0,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Example fault tree: FaultTree1"]
["TOP AND G1 G2 B1 B2"]
["G1 OR B3 B4"]
["G2 AND B5 B6"]
[]
[]
["Here comes FT for initiating event: InitTree"]
["TOP AND B1 G"]
["G OR B2 B3 B4"]
[]
["Here comes FT for barrier: bTree"]
["TOP AND B5 G"]
["G OR B6 B7 B2"]

{"sheet":"Parameters","index":1,"n_rows":9,"n_cols":7,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"lambda","tau","q","Beta"]
["PSW",9.9999999999999995E-7,4380,null,0.1,null,"PSW"]
["PSD",5.0000000000000004E-6,8760,null,0.03,null,"PSD"]
["LU",1E-4,null,1E-4,null,null,"LU"]
["Init",3.0000000000000001E-3,null,null,null,null,"Init"]
["PSV",7.9999999999999996E-6,8760,null,0.1,null,"PSV"]
["RD",null,null,"E-03",null,null,"RD"]

{"sheet":"FTA's","index":2,"n_rows":10,"n_cols":9,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["PSD system, fault tree: PSDTree"]
["TOP OR PSDV LU PSW",null,null,null,null,null,null,null,"FTA without \"Common\" component accross PSD / PSV"]
["PSDV OR PSDC PSDI Common"]
["PSDI AND PSD1 PSD2"]
["PSW OR PSWC PSWI"]
["PSWI AND PSW1 PSW2"]
[]
["PSV system, fault tree: PSVTree"]
["TOP OR PSVC PSVV Common"]
["PSVV AND PSV1 PSV2"]

{"sheet":"ETA","index":3,"n_rows":21,"n_cols":1,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["\u0081 Controlled shutdown, no gas “lost”"]
["\u0082  Gas relieved to flare"]
["\u0083 Gas flowing out of rupture disc"]
["\u0084 Rupture or explosion of separator"]