{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["Fo","FTAsymbols","systemDocumentation","Qo","FTA Drawing","SystemInfo","Reliability data","Sheet1","Minimal cut sets"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":11,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Fo","index":0,"n_rows":3,"n_cols":2,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["Top Event Frequency"]
[]
["F0 =",1.4375390018173204E-15]

{"sheet":"FTAsymbols","index":1,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["TOPP","Ikke nedstengning",null,0,"OR",1]
["LS","Logisk enhet feiler","TOPP",1,"BASIC"]
["FT_PT","PT og FT feiler begge","TOPP",1,"AND"]
["V","Begge ventiler feiler","TOPP",1,"AND"]
["FT","Strømningsgivere feiler ","FT_PT",3,"2ooN"]
["PT","Trykkgivere feiler","FT_PT",3,"2ooN"]
["FT1","Strømningsgiver 1 feiler","FT",5,"BASIC"]
["FT2","Strømningsgiver 2 feiler","FT",5,"BASIC"]
["FT3","Strømningsgiver 3 feiler","FT",5,"BASIC"]
["PT1","Trykkgiver 1 feiler","PT",6,"BASIC"]
["PT2","Trykkgiver 2 feiler","PT",6,"BASIC"]
["PT3","Trykkgiver 3 feiler","PT",6,"BASIC"]
["V1","Ventil 1 feiler","V",4,"BASIC"]
["V2","Ventil 2 feiler","V",4,"BASIC"]

{"sheet":"systemDocumentation","index":2,"n_rows":7,"n_cols":2,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["Function/Sub/variable","Description"]
["LoadNodes","Laster inn symboler i intern struktur fra WS: \"FTAsymbols\""]
["symbolsToScreen","Sletter symboler på skjermen, tenger opp symboler fra intern struktur. Default lastes symbolene fra \"FTAsymbols\""]
["WorksheetOff","Flagg som settes TRUE / FALSE; TRUE = Reliability Data WS kan endres uten at det trigger \"OnCellModified\""]
["loadRelData","Leser data fra WS: \"Reliability data\" inn i interne strukturer"]
["openFTADrawing","Åpner \"tegneflata\", kun en gang. Må kalles flere ganger dersom programmet henger."]
["SaveDrawing","Skriver tilbake symbolene til WS: FTAsymbols"]

{"sheet":"Qo","index":3,"n_rows":3,"n_cols":2,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["Top event probability"]
[]
["Q0 =",0]

{"sheet":"FTA Drawing","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"SystemInfo","index":5,"n_rows":22,"n_cols":8,"rows_kept":22,"cut":false,"hidden":false,"merged":[]}
["Gates","Data types",null,null,null,"C:\\Users\\jvatn\\OneDrive - NTNU\\NTNU-Courses\\PK6018\\PK6018_Eksamen_2021.fta"]
["AND","Repairable",null,null,null,"C:\\Users\\jvatn\\OneDrive - NTNU\\NTNU-Projects\\Programmering\\FTA_Drawing"]
["OR","Non repairable",null,null,null,3]
["1ooN","On demand",null,null,null,{"$f":"nLines*0.333","v":0.99900000000000011}]
["2ooN","Proof test"]
["3ooN","Frequency"]
["4ooN"]
["5ooN"]
["6ooN"]
["7ooN"]
["8ooN"]
["9ooN"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,{"$f":"1-H19","v":1}]

{"sheet":"Reliability data","index":6,"n_rows":1,"n_cols":7,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["Basic event","Compnent type","Lambda","Tau","MDT","OnDemand","Add. Info"]

{"sheet":"Sheet1","index":7,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Minimal cut sets","index":8,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Minimal cut sets"]
[]
["{LS}"]
["{V2,V1}"]
["{PT2,PT1,FT2,FT1}"]
["{PT3,PT2,FT3,FT2}"]
["{PT2,PT1,FT3,FT1}"]
["{PT2,PT1,FT3,FT2}"]
["{PT3,PT1,FT2,FT1}"]
["{PT3,PT2,FT2,FT1}"]
["{PT3,PT1,FT3,FT1}"]
["{PT3,PT2,FT3,FT1}"]
["{PT3,PT1,FT3,FT2}"]